**MF-P5068 M-003927-M**

|  |  |  |
| --- | --- | --- |
| **Multifaster 8 lines: Male plate - 8 housings 3/8".** |  | **Application** |

**4**

|  |
| --- |
|  |

Technical Specifications

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Size | | | Working Pressure | | Flow Rate | Spillage | Burst pressure (MPa & psi) | | | | | |
| dash | mm | inch | (MPa) | (psi) | (l/min) | (ml) | Male | | Female | | Male + Female | |
| 06 | 10 | 3/8 ‘’ | 25 | 3626 | 40 | 0,01 | 100 | 14504 | 100 | 14504 | 100 | 14504 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Materials | **Alluminium; Steel** |  | Valve Type | **Flat** |
| Seals | **NBR; PUR** |  | Connection | **Lever** |
| Working temperatures | **-25 °C to 100 °C**  **-13 F° to 212 F°** |  | Disconnection | **Lever** |
| Surface treatment | **MATE 500 (CRlll); Paint** |  | Connection Under Pressure | **Allowed Residual** |

**Mobile Plate**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | **Housing**  **size** | | | **Thread**  **Type** | | | **Thread**  **Standard** | | | **Thread**  **size** | | **Component Type** | | |  | |
| **Hou.1** | 3/8” | | | 2/ METRIC | | | METRIC "L" MALE | | | 22x1.5 | | | Coupling | | |  | | | |
| **Hou.2** | 3/8” | | | 2/ METRIC | | | METRIC "L" MALE | | | 22x1.5 | | | Coupling | | |  | | | |
| **Hou.3** | 3/8” | | | 2/ METRIC | | | METRIC "L" MALE | | | 22x1.5 | | | Coupling | | |  | | | |
| **Hou.4** | 3/8” | | | 2/ METRIC | | | METRIC "L" MALE | | | 22x1.5 | | | Coupling | | |  | | | |
| **Hou.5** | 3/8” | | | 2/ METRIC | | | METRIC "L" MALE | | | 22x1.5 | | | Coupling | | |  | | | |
| **Hou.6** | 3/8” | | | 2/ METRIC | | | METRIC "L" MALE | | | 22x1.5 | | | Coupling | | |  | | | |
| **Hou.7** | | 3/8” | | | 2/ METRIC | | | METRIC "L" MALE | | | 22x1.5 | | | | Coupling | | |  | | |
| **Hou.8** | | 3/8” | | | 2/ METRIC | | | METRIC "L" MALE | | | 22x1.5 | | | | Coupling | | |  | | |

**Thread chart**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  |  |  |
|  |  |  |  |  |

**Couplings spare parts Plate spare parts**

|  |  |  |
| --- | --- | --- |
|  | **Housing**  **size** | **Spare**  **Part code** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  | | --- | --- | --- | | **Component** | | **Spare**  **Part code** | | **Male plate** | KIT VP8 (SCREWS), KIT GP4 (PINS) | | |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Hou.1** | | 3/8” | | KIT3FNP38-2/22M | |
| **Hou.2** | | 3/8” | | KIT3FNP38-2/22M | |
| **Hou.3** | 3/8” | | KIT3FNP38-2/22M | |
| **Hou.4** | | 3/8” | | KIT3FNP38-2/22M |
| **Hou.5** | | 3/8” | | KIT3FNP38-2/22M |
| **Hou.6** | | 3/8” | | KIT3FNP38-2/22M |
| **Hou.7** | | 3/8” | | KIT3FNP38-2/22M |
| **Hou.8** | | 3/8” | | KIT3FNP38-2/22M |