**MF-P5065 M-004167-M**

|  |  |  |
| --- | --- | --- |
| **Multifaster 5 lines: Male plate - 3 housings 1/4" - 2 housings 3/8".** |  | **Application** |

**4**

|  |
| --- |
|  |

 Technical Specifications

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Size | Working Pressure | Flow Rate | Spillage | Burst pressure (MPa & psi)  |
| dash | mm | inch | (MPa) | (psi) | (l/min) | (ml) | Male | Female | Male + Female |
| 04 | 6.3 | 1/4 ‘’ | 25 | 3626 | 20 | 0,008 | 100 | 14504 | 100 | 14504 | 100 | 14504 |
| 06 | 10 | 3/8 ‘’ | 25 | 3626 | 40 | 0,01 | 100 | 14504 | 100 | 14504 | 100 | 14504 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Materials | **Alluminium; Steel** |  | Valve Type | **Flat** |
| Seals | **NBR; PUR** |  | Connection | **Lever** |
| Working temperatures | **-25 °C to 100 °C****-13 F° to 212 F°** |  | Disconnection | **Lever** |
| Surface treatment | **MATE 500 (CRlll); Paint** |  | Connection Under Pressure | **Allowed Residual** |

**Mobile Plate**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | **Housing** **size** | **Thread** **Type** | **Thread****Standard** | **Thread****size** | **ComponentType** |  |
| **Hou.1** | 3/8” | 0/ SAE | SAE ORB FEMALE | 1/2" | Coupling |  |
| **Hou.2** | 3/8” |  |  |  | Plug |  |
| **Hou.3** | 1/4” | 0/ SAE | SAE ORB FEMALE | 1/4" | Coupling |  |
| **Hou.4** | 1/4” | 0/ SAE | SAE ORB FEMALE | 1/4" | Coupling |  |
| **Hou.5** | 1/4” | 0/ SAE | SAE ORB FEMALE | 1/4" | Coupling |  |

**Thread chart**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  |  |  |
|  |  |  |  |  |

**Couplings spare parts Plate spare parts**

|  |  |  |
| --- | --- | --- |
|  |  **Housing**  **size** |  **Spare** **Part code** |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|

|  |  |
| --- | --- |
| **Component** |  **Spare** **Part code** |
| **Male plate** | KIT VP4 (SCREWS), KIT GP4 (PINS) |

 |  |

|  |  |  |
| --- | --- | --- |
| **Hou.1** | 3/8” |  KIT3FNP38-12SM |
| **Hou.2** | 3/8” |  KIT TSP 38 M |
| **Hou.3** | 1/4” |  - |
| **Hou.4** | 1/4” | - |
| **Hou.5** | 1/4” | - |