**MF-P510 A F-004186-F**

|  |  |  |
| --- | --- | --- |
| **Multifaster 4 lines: Male plate - 2 housings 1/2" - 2 housings 3/4".** |  | **Application** |

**4**

|  |  |
| --- | --- |
|  |  |

 Technical Specifications

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Size | Working Pressure | Flow Rate | Spillage | Burst pressure (MPa & psi)  |
| dash | mm | inch | (MPa) | (psi) | (l/min) | (ml) | Male | Female | Male + Female |
| 08 | 12,5 | 1/2 ‘’ | 20 | 2900 | **MultiGrease** | 60 | 8702 | 100 | 14504 | 60 | 8702 |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 12 | 20 | 3/4 ‘’ | 25 | 3626 | 105 | 0,02 | 100 | 14504 | 100 | 14504 | 100 | 14504 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Materials | **Alluminium; Steel** |  | Valve Type | **Flat** |
| Seals | **NBR; PUR** |  | Connection | **Lever** |
| Working temperatures | **-25 °C to 100 °C****-13 F° to 212 F°** |  | Disconnection | **Lever** |
| Surface treatment | **MATE 500 (CRlll); Paint** |  | Connection Under Pressure | **Allowed Residual** |

**Fixed Plate**

**Lever Type:** Left short lever, flat handle, left safety lock

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | **Housing** **size** | **Thread** **Type** | **Thread****Standard** | **Thread****size** | **ComponentType** |  |
| **Hou.1** | 3/4” | --/ BSP | BSP FEMALE | 3/4" | Coupling |  |
| **Hou.2** | 1/2” | --/ BSP | BSP FEMALE | 1/8" | MultiGrease | 7 PINS, rated current: 13 A |
| **Hou.3** | 1/2” |  |  |  | Electrical connector | 7 PINS, rated current: 13 A |
| **Hou.4** | 3/4” | --/ BSP | BSP FEMALE | 3/4" | Coupling |  |

**Thread chart**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  |  |  |
|  |  |  |  |  |

**Couplings spare parts Plate spare parts**

|  |  |  |
| --- | --- | --- |
|  |  **Housing**  **size** |  **Spare** **Part code** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |  |
| --- | --- |
| **Component** |  **Spare** **Part code** |
| **Female plate** | KIT SP5 S (SAFETY LOCK) |
| **Lever** | KIT L3P412 B |

 |  |

|  |  |  |
| --- | --- | --- |
| **Hou.1** | 3/4” |  KIT2FNB34GAS F |
| **Hou.2** | 1/2” |  KIT2FNGS12 AAF |
| **Hou.3** | 1/2” |  KIT SPEL08-7F |
| **Hou.4** | 3/4” | KIT2FNB34GAS F |