**MF-P508 A F-004625-F**

|  |  |  |
| --- | --- | --- |
| **Multifaster 4 lines: Female plate - 4 housings 1/2".** |  | **Application** |

**4**

|  |  |
| --- | --- |
|  |  |

 Technical Specifications

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Size | Working Pressure | Flow Rate | Spillage | Burst pressure (MPa & psi)  |
| dash | mm | inch | (MPa) | (psi) | (l/min) | (ml) | Male | Female | Male + Female |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| - | - | - | - | - | - | - | - | - | - | - | - | - |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Materials | **Alluminium; Steel** |  | Valve Type | **Flat** |
| Seals | **NBR; PUR** |  | Connection | **Lever** |
| Working temperatures | **-25 °C to 100 °C****-13 F° to 212 F°** |  | Disconnection | **Lever** |
| Surface treatment | **MATE 500 (CRlll); Paint** |  | Connection Under Pressure | **Allowed Residual** |

**Fixed Plate**

**Lever Type:** Right short lever, right safety lock, flat handle, better grip

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | **Housing** **size** | **Thread** **Type** | **Thread****Standard** | **Thread****size** | **ComponentType** |  |
| **Hou.1** | 1/2” |  |  |  | Electrical connector | 7 PINS, rated current: 13 A |
| **Hou.2** | 1/2” |  |  |  | Empty |  |
| **Hou.3** | 1/2” |  |  |  | Empty |  |
| **Hou.4** | 1/2” |  |  |  | Electrical connector | 7 PINS, rated current: 13 A |

Please, note that this is a configuration Faster does not recommend.
This selection might cause an unbalanced hydraulic load.

**Thread chart**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  |  |  |
|  |  |  |  |  |

**Couplings spare parts Plate spare parts**

|  |  |  |
| --- | --- | --- |
|  |  **Housing**  **size** |  **Spare** **Part code** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |  |
| --- | --- |
| **Component** |  **Spare** **Part code** |
| **Female plate** | KIT SP5 S (SAFETY LOCK) |
| **Lever** | - |

 |  |

|  |  |  |
| --- | --- | --- |
| **Hou.1** | 1/2” |  KIT SPEL08-7F |
| **Hou.2** | 1/2” |  - |
| **Hou.3** | 1/2” |  - |
| **Hou.4** | 1/2” | KIT SPEL08-7F |