**MF-P508 A F-004764-F**

|  |  |  |
| --- | --- | --- |
| **Multifaster 4 lines: Male plate - 2 housings 1/2" - 2 housings 3/4".** |  | **Application** |

**4**

|  |  |
| --- | --- |
|  |  |

Technical Specifications

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Size | | | Working Pressure | | Flow Rate | Spillage | Burst pressure (MPa & psi) | | | | | |
| dash | mm | inch | (MPa) | (psi) | (l/min) | (ml) | Male | | Female | | Male + Female | |
| 08 | 12,5 | 1/2 ‘’ | 25 | 3626 | 70 | 0,01 | 100 | 14504 | 100 | 14504 | 100 | 14504 |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 12 | 20 | 3/4 ‘’ | 25 | 3626 | 105 | 0,02 | 100 | 14504 | 100 | 14504 | 100 | 14504 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Materials | **Alluminium; Steel** |  | Valve Type | **Flat** |
| Seals | **NBR; PUR** |  | Connection | **Lever** |
| Working temperatures | **-25 °C to 100 °C**  **-13 F° to 212 F°** |  | Disconnection | **Lever** |
| Surface treatment | **MATE 500 (CRlll); Paint** |  | Connection Under Pressure | **Allowed Residual** |

**Fixed Plate**

**Lever Type:** "U" long lever, left safety lock

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | **Housing**  **size** | | **Thread**  **Type** | | **Thread**  **Standard** | | **Thread**  **size** | | **Component Type** | |  |
| **Hou.1** | 3/4” | | --/ BSP | | BSP FEMALE | | 3/4" | | Coupling | | 7 PINS, rated current: 13 A | | |
| **Hou.2** | 1/2” | | 13/ SAE | | SAE JIC 37° MALE | | 1/2" | | Coupling | |  | | |
| **Hou.3** | 1/2” | |  | |  | |  | | Electrical connector | | 3 PINS, rated current: 13 A | | |
| **Hou.4** | 3/4” | | --/ BSP | | BSP FEMALE | | 3/4" | | Coupling | |  | | |

**Thread chart**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  |  |  |
|  |  |  |  |  |

**Couplings spare parts Plate spare parts**

|  |  |  |
| --- | --- | --- |
|  | **Housing**  **size** | **Spare**  **Part code** |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  | | --- | --- | --- | --- | | **Component** | | | **Spare**  **Part code** | | **Female plate** | KIT VP8 (SCREWS), KIT SP5 S (SAFETY LOCK) | | | | | **Lever** | | - | | | |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Hou.1** | | 3/4” | | KIT2FNB34GAS F | |
| **Hou.2** | | 1/2” | | KIT2FNB1213/12S | |
| **Hou.3** | 1/2” | | KIT SPEL08-3F | |
| **Hou.4** | | 3/4” | | KIT2FNB34GAS F |