|  |  |  |
| --- | --- | --- |
| **Multifaster 8 lines: Male plate - 8 housings 1/2".** |  | **Application**  **ico_agriculture-full-pos** |

**MF-P808 M-005231-M**

**4**

|  |
| --- |
|  |

Technical Specifications

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Size | | | Working Pressure | | Flow Rate | Spillage | Burst pressure (MPa & psi) | | | | | |
| dash | mm | inch | (MPa) | (psi) | (l/min) | (ml) | Male | | Female | | Male + Female | |
| 08 | 12,5 | 1/2 ‘’ | 25 | 3626 | 70 | 0,01 | 100 | 14504 | 100 | 14504 | 100 | 14504 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Materials | **Aluminium; Steel** |  | Valve Type | **Flat** |
| Seals |  |  | Connection | **Lever** |
| Working temperatures | **-25°C to 100°C**  **-13 F° to 212 F°** |  | Disconnection | **Lever** |
| Surface treatment | **CARBON STEEL (CRlll); Paint** |  | Connection Under Pressure |  |

**Mobile Plate**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | **Housing**  **size** | | | **Thread**  **Type** | | | **Thread**  **Standard** | | | **Thread**  **size** | | **Component Type** | | |  | |
| **Hou.1** | 1/2” | | | 3/ METRIC | | | METRIC "S" MALE | | | 24x1.5 | | | Coupling | | |  | | | |
| **Hou.2** | 1/2” | | |  | | |  | | |  | | | Electrical connector | | | 7 PINS, rated current: 13 A | | | |
| **Hou.3** | 1/2” | | | 3/ METRIC | | | METRIC "S" MALE | | | 24x1.5 | | | Coupling | | |  | | | |
| **Hou.4** | 1/2” | | |  | | |  | | |  | | | Empty | | |  | | | |
| **Hou.5** | 1/2” | | |  | | |  | | |  | | | Empty | | |  | | | |
| **Hou.6** | 1/2” | | | 2/ METRIC | | | METRIC "L" MALE | | | 16x1.5 | | | Coupling | | |  | | | |
| **Hou.7** | | 1/2” | | |  | | |  | | |  | | | | Electrical connector | | | 7 PINS, rated current: 13 A | | |
| **Hou.8** | | 1/2” | | | 2/ METRIC | | | METRIC "L" MALE | | | 16x1.5 | | | | Coupling | | |  | | |

Please, note that this is a configuration Faster does not recommend.  
This selection might cause an unbalanced hydraulic load.

**Thread chart**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  |  |  |
|  |  |  |  |  |

**Couplings spare parts Plate spare parts**

|  |  |  |
| --- | --- | --- |
|  | **Housing**  **size** | **Spare**  **Part code** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  | | --- | --- | --- | | **Component** | | **Spare**  **Part code** | | **Male plate** | KIT VP8 (SCREWS), KIT GP8 (PINS) | | |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Hou.1** | | 1/2” | | KIT3FNP12-3/24M | |
| **Hou.2** | | 1/2” | | KIT SPEL08-7M | |
| **Hou.3** | 1/2” | | KIT3FNP12-3/24M | |
| **Hou.4** | | 1/2” | | - |
| **Hou.5** | | 1/2” | | - |
| **Hou.6** | | 1/2” | | - |
| **Hou.7** | | 1/2” | | KIT SPEL08-7M |
| **Hou.8** | | 1/2” | | - |