|  |  |  |
| --- | --- | --- |
| **Multifaster 6 lines: Female plate - 2 housings 1/2" - 4 housings 3/4"'.** |  | **Application****ico_industrial-full-pos** |

**MF-P6I F-005539-F**

**4**

|  |  |
| --- | --- |
|  |  |

Technical Specifications

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Size | Working Pressure | Flow Rate | Spillage | Burst pressure (MPa & psi)  |
| dash | mm | inch | (MPa) | (psi) | (l/min) | (ml) | Male | Female | Male + Female |
| 08 | 12,5 | 1/2 ‘’ | 20 | 2900 | **MultiGrease** | 60 | 8702 | 100 | 14504 | 60 | 8702 |
| 12 | 20 | 3/4 ‘’ | 25 | 3626 | 105 | 0,02 | 100 | 14504 | 100 | 14504 | 100 | 14504 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Materials | **Aluminium; Steel** |  | Valve Type | **Flat** |
| Seals |  |  | Connection | **Lever** |
| Working temperatures | **-25°C to 100°C****-13 F° to 212 F°** |  | Disconnection | **Lever** |
| Surface treatment | **CARBON STEEL (CRlll); Paint** |  | Connection Under Pressure |  |

**Fixed Plate**

**Lever Type:** "U" long lever, left safety lock

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | **Housing** **size** | **Thread** **Type** | **Thread****Standard** | **Thread****size** | **ComponentType** |  |
| **Hou.1** | 3/4” |  |  |  | Empty |  |
| **Hou.2** | 3/4” |  |  |  | Empty |  |
| **Hou.3** | 1/2” | --/ BSP | BSP FEMALE | 1/8" | MultiGrease |  |
| **Hou.4** | 1/2” | --/ BSP | BSP FEMALE | 1/8" | MultiGrease |  |
| **Hou.5** | 3/4” | --/ NPT | NPT\_FEMALE | 3/4" | Coupling |  |
| **Hou.6** | 3/4” |  |  |  | Empty |  |

Please, note that this is a configuration Faster does not recommend.
This selection might cause an unbalanced hydraulic load.

**Thread chart**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  |  |  |
|  |  |  |  |  |

**Couplings spare parts Plate spare parts**

|  |  |  |
| --- | --- | --- |
|  |  **Housing**  **size** |  **Spare** **Part code** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |  |
| --- | --- |
| **Component** |  **Spare** **Part code** |
| **Female plate** | KIT TA P8 (CAP), KIT SP5 S (SAFETY LOCK) |
| **Lever** | KIT LP10A |

 |  |

|  |  |  |
| --- | --- | --- |
| **Hou.1** | 3/4” |  - |
| **Hou.2** | 3/4” |  - |
| **Hou.3** | 1/2” |  KIT2FNGS12 AAF |
| **Hou.4** | 1/2” | KIT2FNGS12 AAF |
| **Hou.5** | 3/4” | KIT2FNB34NPT F |
| **Hou.6** | 3/4” | - |