|  |  |  |
| --- | --- | --- |
| **Multifaster 4 lines: Female plate - 4 housings 3/4".** |  | **Application****ico_industrial-full-pos** |

**MF-P412 F-005688-F**

**4**

|  |  |
| --- | --- |
|  |  |

Technical Specifications

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Size | Working Pressure | Flow Rate | Spillage | Burst pressure (MPa & psi)  |
| dash | mm | inch | (MPa) | (psi) | (l/min) | (ml) | Male | Female | Male + Female |
| 12 | 20 | 3/4 ‘’ | 25 | 3626 | 105 | 0,02 | 100 | 14504 | 100 | 14504 | 100 | 14504 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Materials | **Aluminium; Steel** |  | Valve Type | **Flat** |
| Seals |  |  | Connection | **Lever** |
| Working temperatures | **-25°C to 100°C****-13 F° to 212 F°** |  | Disconnection | **Lever** |
| Surface treatment | **CARBON STEEL (CRlll); Paint** |  | Connection Under Pressure |  |

**Fixed Plate**

**Lever Type:** Left short lever, left safety lock

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | **Housing** **size** | **Thread** **Type** | **Thread****Standard** | **Thread****size** | **ComponentType** |  |
| **Hou.1** | 3/4” | 3/ METRIC | METRIC "S" MALE | 30x2 | Coupling |  |
| **Hou.2** | 3/4” | 3/ METRIC | METRIC "S" MALE | 30x2 | Coupling |  |
| **Hou.3** | 3/4” | 3/ METRIC | METRIC "S" MALE | 30x2 | Coupling |  |
| **Hou.4** | 3/4” | 3/ METRIC | METRIC "S" MALE | 30x2 | Coupling |  |

**Thread chart**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  |  |  |
|  |  |  |  |  |

**Couplings spare parts Plate spare parts**

|  |  |  |
| --- | --- | --- |
|  |  **Housing**  **size** |  **Spare** **Part code** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |  |
| --- | --- |
| **Component** |  **Spare** **Part code** |
| **Female plate** | KIT SP5 S (SAFETY LOCK) |
| **Lever** | KIT L3P510 |

 |  |

|  |  |  |
| --- | --- | --- |
| **Hou.1** | 3/4” |  KIT2FNB34-3/30F |
| **Hou.2** | 3/4” |  KIT2FNB34-3/30F |
| **Hou.3** | 3/4” |  KIT2FNB34-3/30F |
| **Hou.4** | 3/4” | KIT2FNB34-3/30F |