|  |  |  |
| --- | --- | --- |
| **Multifaster 2 lines: Female plate - 2 housings 3/8".** |  | **Application****ico_industrial-full-pos** |

**MF-PB06 FD-005570-F**

**4**

|  |  |
| --- | --- |
|  |  |

Technical Specifications (Stainless Steel)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Size | Working Pressure | Flow Rate | Spillage | Burst pressure (MPa & psi)  |
| dash | mm | inch | (MPa) | (psi) | (l/min) | (ml) | Male | Female | Male + Female |
| 06 | 10 | 3/8 ‘’ | 25 | 3626 | 40 | 0,01 | 100 | 14504 | 100 | 14504 | 100 | 14504 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Materials | **; Stainless steel****Aluminium; Steel** |  | Valve Type | **Flat** |
| Seals | **VITON** |  | Connection | **Lever** |
| Working temperatures | **-22°C to 200°C****-4 F° to 392 F°** |  | Disconnection | **Lever** |
| Surface treatment | **CARBON STEEL (CRlll); Paint** |  | Connection Under Pressure | **Not allowed for Stainless steel** |

**Fixed Plate**

**Lever Type:** Right short lever, flat handle, right safety lock

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | **Housing** **size** | **Thread** **Type** | **Thread****Standard** | **Thread****size** | **ComponentType** |  |
| **Hou.1** | 3/8” | --/ BSP | BSP FEMALE | 3/8" | Coupling |  |
| **Hou.2** | 3/8” | --/ BSP | BSP FEMALE | 3/8" | Coupling |  |

**Thread chart**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  |  |  |
|  |  |  |  |  |

**Couplings spare parts Plate spare parts**

|  |  |  |
| --- | --- | --- |
|  |  **Housing**  **size** |  **Spare** **Part code** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |  |
| --- | --- |
| **Component** |  **Spare** **Part code** |
| **Female plate** | KIT GP4 (PINS), KIT SP5 S (SAFETY LOCK), KIT TA PB06 (CAP) |
| **Lever** | KIT LPB06 LI |

 |  |

|  |  |  |
| --- | --- | --- |
| **Hou.1** | 3/8” |  KIT2FNB38G F2V |
| **Hou.2** | 3/8” |  KIT2FNB38G F2V |