|  |  |  |
| --- | --- | --- |
| **Multifaster 4 lines: Female plate - 4 housings 3/8".** |  | **Application**  **ico_agriculture-full-pos** |

**MF-P506 F-005124-F**

**4**

|  |  |
| --- | --- |
|  |  |

Technical Specifications (Stainless Steel)

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Size | | | Working Pressure | | Flow Rate | Spillage | Burst pressure (MPa & psi) | | | | | |
| dash | mm | inch | (MPa) | (psi) | (l/min) | (ml) | Male | | Female | | Male + Female | |
| 06 | 10 | 3/8 ‘’ | 25 | 3626 | 40 | 0,01 | 100 | 14504 | 100 | 14504 | 100 | 14504 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Materials | **; Stainless steel**  **Aluminium; Steel** |  | Valve Type | **Flat** |
| Seals | **VITON** |  | Connection | **Lever** |
| Working temperatures | **-22°C to 200°C**  **-4 F° to 392 F°** |  | Disconnection | **Lever** |
| Surface treatment | **CARBON STEEL (CRlll); Paint** |  | Connection Under Pressure | **Not allowed for Stainless steel** |

**Fixed Plate**

**Lever Type:** "U" lever, left safety lock, metal handle

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | **Housing**  **size** | | **Thread**  **Type** | | **Thread**  **Standard** | | **Thread**  **size** | | **Component Type** | |  |
| **Hou.1** | 3/8” | | --/ BSP | | BSP FEMALE | | 3/8" | | Coupling | |  | | |
| **Hou.2** | 3/8” | | --/ BSP | | BSP FEMALE | | 3/8" | | Coupling | |  | | |
| **Hou.3** | 3/8” | | --/ BSP | | BSP FEMALE | | 3/8" | | Coupling | |  | | |
| **Hou.4** | 3/8” | | --/ BSP | | BSP FEMALE | | 3/8" | | Coupling | |  | | |

**Thread chart**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  |  |  |
|  |  |  |  |  |

**Couplings spare parts Plate spare parts**

|  |  |  |
| --- | --- | --- |
|  | **Housing**  **size** | **Spare**  **Part code** |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  | | --- | --- | --- | --- | | **Component** | | | **Spare**  **Part code** | | **Female plate** | KIT VP4 (SCREWS), KIT SP5 S (SAFETY LOCK) | | | | | **Lever** | | KIT LP506 | | | |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Hou.1** | | 3/8” | | KIT2FNB38G F2V | |
| **Hou.2** | | 3/8” | | KIT2FNB38G F2V | |
| **Hou.3** | 3/8” | | KIT2FNB38G F2V | |
| **Hou.4** | | 3/8” | | KIT2FNB38G F2V |